## Greenhouse Facilities Checklist

|  |  |  |  |
| --- | --- | --- | --- |
| Electrical panels covered | Yes | No | N/A |
| All electrical junction boxes are covered |  |  |  |
| Outlets are waterproof |  |  |  |
| Outlets are protected by GFCI circuits (shock hazards) |  |  |  |
| Extension cords are grounded and in good conditions |  |  |  |
| Pesticides and chemicals are in locked storage with waterproof shelves |  |  |  |
| All chemicals are clearly labeled |  |  |  |
| Eye wash supplies/station are available and clearly marked |  |  |  |
| Pesticide application logs are kept and easily accessible |  |  |  |
| SDS sheets are available and clearly marked for all materials |  |  |  |
| Personal Protective Equipment (PPE) is provided (see chemical safety) |  |  |  |
| Aisles are kept clear |  |  |  |
| Facility is free of trip hazards such as hoses and electrical cords |  |  |  |
| Walkways are non skid (not slippery) |  |  |  |
| Fans and other equipment are well guarded |  |  |  |
| Fire extinguishers are available, easily located, serviced annually |  |  |  |
| Compressed gas cylinder are properly stored (restrained) |  |  |  |
| Shade cloth is fire resistant and 3 feet from all combustible sources like fan motors and heaters |  |  |  |